{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"images":14,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"merged":[[13,0,13,8],[14,0,14,8],[27,0,27,8],[45,0,45,8],[65,0,65,8],[79,0,79,8]],"flags":["formulas_cached_only"]}
{"$rows_empty":13}
["Светодиодные светильники LEDEL"]
["Офисные светильники "]
["Наименование","Стекло","Свето диод","Потреб ление   ","Световой поток","Температура  свечения","Габаритные размеры   ДхШхВ                            ","Масса с упаков.","Цена, руб."]
["L-OFFICE 25/3000/32 Встраиваемый","MicroPrisma","CREE","32 Вт","3000 Лм","5000 К"," 595Х595х40 мм","4,0 кг",7900]
["L-OFFICE 25/3000/32 Накладной (хром)","MicroPrisma","CREE","32 Вт","3000 Лм","5000 К","600Х600х50 мм","4,0 кг",10000]
["L-SCHOOL 24/2900/30 Накладной","MicroPrisma","CREE","30 Вт","2900 Лм","5000 К","1200Х200х45 мм","3,5 кг",7900]
{"$rows_empty":8}
["Уличные светильники "]
["Наименование","Стекло","Свето диод","Потреб ление  ","Световой поток","Температура  свечения","Габаритные размеры               ВхДхШ       ","Масса с упаков.","Цена, руб."]
["SVETECO 24/2688/30              IP67","Поликарбонат","OSRAM","30 Вт","2688 Лм","5500 К","     305x519x92 мм           ","4,5 кг",9000]
["SVETECO 24/3300/40              IP67","Поликарбонат","OSRAM","40 Вт","3300 Лм","5500 К","     305x519x92 мм             ","4,5 кг",9450]
["SVETECO 48/5376/60              IP67","Поликарбонат","OSRAM","60 Вт","5376 Лм","5500 К","    120x519x181 мм          ","6,5 кг",15000]
["SVETECO 48/6624/80              IP67","Поликарбонат","OSRAM","80 Вт","6624 Лм","5500 К","    120x519x181 мм            "," 6,5 кг",15750]
["SVETECO 72/9936/120            IP67","Поликарбонат","OSRAM","120 Вт","9936 Лм","5500 К","    120x519x270 мм            "," 9,0 кг",20000]
["SVETECO 96/10752/120          IP67","Поликарбонат","OSRAM","120 Вт","10752 Лм","5500 К","    120x519x360 мм            ","12,5кг",25000]
["SVETECO 96/13248/160          IP67","Поликарбонат","OSRAM","160 Вт","13248 Лм","5500 К","    120x519x360 мм             ","12,5кг",26000]
{"$rows_empty":9}
["Промышленные светильники "]
["Наименование","Стекло","Свето диод","Потреб ление  ","Световой поток","Температура  свечения","Габаритные размеры          ВхДхШ       ","Масса с упаков.","Цена, руб."]
["L-INDUSTRY 36/4390/45             IP67","На выбор","CREE","45 Вт","4390 Лм","5500 К","80х1064x100 мм              ","6,5 кг ",10900]
["L-INDUSTRY 36/4032/45             IP67","Поликарбонат","OSRAM","45 Вт","4032 Лм","5500 К","80х1064x100 мм              ","6,5 кг ",11950]
["L-INDUSTRY 48/5800/60             IP67","На выбор","CREE","60 Вт","5800 Лм","5500 К","80х1064x100 мм              ","6,5 кг ",14400]
["L-INDUSTRY АЗС 48/5800/60     IP67","Поликарбонат","CREE","60 Вт","5800 Лм","5500 К","  103х551х220 мм","6,5 кг ",15000]
["L-INDUSTRY 72/8780/90             IP67","Поликарбонат","CREE","90 Вт","8780 Лм","5500 К","  120x519x270 мм            ","9,0 кг ",17600]
["L-INDUSTRY 72/8064/90             IP67","Поликарбонат","OSRAM","90 Вт","8064 Лм","5500 К","  120x519x270 мм            ","9,0 кг ",19500]
["L-INDUSTRY 96/11712/120         IP67","Поликарбонат","СREE","120 Вт","11712 Лм","5500 К","  120x519x360 мм             ","11,5 кг",23400]
["L-INDUSTRY 96/10752/120         IP67","Поликарбонат","OSRAM","120 Вт","10752 Лм","5500 К","  120x519x360 мм             ","11,5 кг",24500]
{"$rows_empty":10}
["Бытовые и ЖКХ светильники "]
["Наименование","Стекло","Свето диод","Потреб ление  ","Световой поток","Температура  свечения","Габаритные размеры           ВхДхШ       ","Масса с упаков.","Цена, руб. "]
["SVETECO     7/870/9                           IP67","Поликарбонат","CREE","9 Вт","   870 Лм","5000 К","70x150х150 мм                           ","0,8 кг",2000]
["SVETECO 8/1000/10 датчик звука   IP67","Поликарбонат","CREE","10 Вт","1000 Лм","5000 К","70x150х150 мм                           ","0,8 кг",2200]
["L-12/1464/15","Поликарбонат","CREE","15 Вт","1464 Лм","5000 К","96x314x92 мм","2,0 кг",3000]
{"$rows_empty":9}
["Прожекторы "]
["Наименование","Стекло","Свето диод","Потреб ление  ","Световой поток","Температура  свечения","Габаритные размеры           ВхДхШ       ","Масса с упаков.","Цена, руб. "]
["L-BANNER 24/3000/30         IP67","Поликарбонат","CREE","30 Вт","3000 Лм","5500 К","100x320х180 мм                ","4,0 кг",7000]
["L-BANNER 24/3300/40         IP67","Поликарбонат","OSRAM","40 Вт","3300 Лм","5500 К","100x320х180 мм                ","4,0 кг",8250]
["L-BANNER 48/5376/60         IP67","Поликарбонат","OSRAM","60 Вт","5376Лм","5500 К","100х560х180 мм","6,5 кг",15000]
{"$rows_empty":9}
["ООО \"ЭнергоРесурс\"  -  официальный дилер LEDEL "]
["192148, Санкт-Петербург, ул. Седова, д.13, офис 307, тел.: (812) 640-76-36, т/ф.:(812) 640-64-33, моб. (812) 913-66-68"]
["E-mail: energoresurs-spb@bk.ru"]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}